Keywords: **autel battery tester, autel bt608**

Unlike traditional battery testers, Autel MaxiBAS BT608 car battery tester applies future technology “Adaptive Conductance” that can identify low capacity batteries or batteries that are almost completely discharged and thereby reduce battery misdiagnosis. No need to charge and retest, improves battery testing efficiency and accuracy for technicians and DIYers.

* ****Accurate Battery Diagnosis**** Autel MaxiBAS BT608 is a professional analysis tool for testing 6- and 12-volt batteries from 100-3000 CCA, it covers Flooded, AGM, AGM Spiral, EFB and GEL Cell batteries. With the Adaptive Conductance technology, users can get the most accurate test results and minimize the chances of misdiagnosis.
* ****Data Viewing/Printing**** Autel Digital Auto Battery Analyzer BT608 has data review function that enables technician to review the data record, and print out the diagnostic report instantly with the built-in thermal printer, sharing report by email is supported
* ****Full Systems Diagnois**** Autel all systems diagnosis scan tool BT608 is not only a professional battery tester, but also an ideal wireless FULL SYSTEMS scanner.

The Autel BT608 is a touchscreen Battery and Electrical System analyzer featuring Adaptive Conductance, a sophisticated method for analyzing batteries that delivers a more precise evaluation of their cold cranking power and reserve capacity, crucial for assessing battery health. The BT608 can quickly check the battery’s health, register a new battery, and perform in-depth diagnostics on both the battery and electrical system. Its VINscan function quickly identifies the vehicle and battery details. It also allows reading and clearing codes across all vehicle systems, and users can print or share custom reports via Wi-Fi or the integrated thermal printer.